|  |  |  |  |
| --- | --- | --- | --- |
|  | |  | | --- | | **Simulation of borderless\_simplified\_panel\_compression**  **Date: Sunday, May 16, 2021 Designer: Solidworks**  **Study name: compression**  **Analysis type: Static** | | Table of Contents  [Description 1](#_Toc72097594)  [Assumptions 2](#_Toc72097595)  [Model Information 2](#_Toc72097596)  [Study Properties 4](#_Toc72097597)  [Units 5](#_Toc72097598)  [Material Properties 6](#_Toc72097599)  [Loads and Fixtures 8](#_Toc72097600)  [Connector Definitions 8](#_Toc72097601)  [Contact Information 9](#_Toc72097602)  [Mesh information 11](#_Toc72097603)  [Sensor Details 12](#_Toc72097604)  [Resultant Forces 13](#_Toc72097605)  [Beams 13](#_Toc72097606)  [Study Results 14](#_Toc72097607)  [Conclusion 16](#_Toc72097608) | |
| Description No Data |

|  |
| --- |
| Assumptions |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Model Information  |  |  |  |  |  | | --- | --- | --- | --- | --- | | |  | | --- | |  |   ****Model name:** borderless\_simplified\_panel\_compression**  ****Current Configuration:** Default** | | | | | ****Solid Bodies**** | | | | | ****Document Name and Reference**** | ****Treated As**** | ****Volumetric Properties**** | ****Document Path/Date Modified**** | | **Boss-Extrude1** | **Solid Body** | ****Mass:0.0106851 kg****  ****Volume:4.87902e-06 m^3****  ****Density:2,190 kg/m^3****  ****Weight:0.104714 N**** | ****C:\Users\Natha\Desktop\Caltech 2020-2024\NASA\_Big\_Idea\_Challenge\GrabCAD\Current\Mechanical\v4\_Eggdee\Parts\adhesive\_v4.1.SLDPRT****  **May 16 13:19:20 2021** | | **Boss-Extrude1** | **Solid Body** | ****Mass:0.0106851 kg****  ****Volume:4.87902e-06 m^3****  ****Density:2,190 kg/m^3****  ****Weight:0.104714 N**** | ****C:\Users\Natha\Desktop\Caltech 2020-2024\NASA\_Big\_Idea\_Challenge\GrabCAD\Current\Mechanical\v4\_Eggdee\Parts\adhesive\_v4.1.SLDPRT****  **May 16 13:19:20 2021** | | **CirPattern2** | **Solid Body** | ****Mass:0.534853 kg****  ****Volume:0.000212243 m^3****  ****Density:2,520 kg/m^3****  ****Weight:5.24155 N**** | ****C:\Users\Natha\Desktop\Caltech 2020-2024\NASA\_Big\_Idea\_Challenge\GrabCAD\Current\Mechanical\v4\_Eggdee\Simplified\_Parts\bplate\_simplified\_compression\_borderless.SLDPRT****  **May 16 19:51:03 2021** | | **Boss-Extrude1** | **Solid Body** | ****Mass:0.00831385 kg****  ****Volume:5.85483e-06 m^3****  ****Density:1,420 kg/m^3****  ****Weight:0.0814758 N**** | ****C:\Users\Natha\Desktop\Caltech 2020-2024\NASA\_Big\_Idea\_Challenge\GrabCAD\Current\Mechanical\v4\_Eggdee\Simplified\_Parts\pcb\_simplified\_nofillet.SLDPRT****  **May 16 16:25:29 2021** | | **Fillet1** | **Solid Body** | ****Mass:0.0319938 kg****  ****Volume:1.59969e-05 m^3****  ****Density:2,000 kg/m^3****  ****Weight:0.313539 N**** | ****C:\Users\Natha\Desktop\Caltech 2020-2024\NASA\_Big\_Idea\_Challenge\GrabCAD\Current\Mechanical\v4\_Eggdee\Parts\power\_supply\_pcb\_mockup\_v4.2.SLDPRT****  **May 15 11:00:41 2021** | | **Fillet1** | **Solid Body** | ****Mass:0.0269748 kg****  ****Volume:1.89963e-05 m^3****  ****Density:1,420 kg/m^3****  ****Weight:0.264353 N**** | ****C:\Users\Natha\Desktop\Caltech 2020-2024\NASA\_Big\_Idea\_Challenge\GrabCAD\Current\Mechanical\v4\_Eggdee\Simplified\_Parts\separation\_layer\_simplified.SLDPRT****  **May 16 13:10:37 2021** | | **Split Line1** | **Solid Body** | ****Mass:0.0494616 kg****  ****Volume:1.24903e-05 m^3****  ****Density:3,960 kg/m^3****  ****Weight:0.484723 N**** | ****C:\Users\Natha\Desktop\Caltech 2020-2024\NASA\_Big\_Idea\_Challenge\GrabCAD\Current\Mechanical\v4\_Eggdee\Simplified\_Parts\tplate\_simplified.SLDPRT****  **May 16 22:41:33 2021** | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Study Properties  |  |  | | --- | --- | | Study name | compression | | Analysis type | Static | | Mesh type | Solid Mesh | | Thermal Effect: | On | | Thermal option | Include temperature loads | | Zero strain temperature | 298 Kelvin | | Include fluid pressure effects from SOLIDWORKS Flow Simulation | Off | | Solver type | FFEPlus | | Inplane Effect: | Off | | Soft Spring: | Off | | Inertial Relief: | Off | | Incompatible bonding options | Automatic | | Large displacement | Off | | Compute free body forces | On | | Friction | Off | | Use Adaptive Method: | Off | | Result folder | SOLIDWORKS document (C:\Users\Natha\Desktop\Caltech 2020-2024\NASA\_Big\_Idea\_Challenge\GrabCAD\Current\Mechanical\v4\_Eggdee\Simplified\_Parts\5.16\_Compression\_Simplified\_Borderless) | |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Units  |  |  | | --- | --- | | Unit system: | SI (MKS) | | Length/Displacement | mm | | Temperature | Kelvin | | Angular velocity | Rad/sec | | Pressure/Stress | N/m^2 | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Material Properties  |  |  |  | | --- | --- | --- | | ****Model Reference**** | ****Properties**** | ****Components**** | |  | |  |  | | --- | --- | | ****Name:**** | **STYCAST 2850FT/Catalyst 23LV** | | ****Model type:**** | **Linear Elastic Isotropic** | | ****Default failure criterion:**** | **Unknown** | | ****Tensile strength:**** | **1.0549e+08 N/m^2** | | ****Compressive strength:**** | **1.19969e+08 N/m^2** | | ****Elastic modulus:**** | **6.413e+09 N/m^2** | | ****Mass density:**** | **2,190 kg/m^3** | | **SolidBody 1(Boss-Extrude1)(adhesive\_v4.1-1),**  **SolidBody 1(Boss-Extrude1)(adhesive\_v4.1-2)** | | **Curve Data:N/A** | | | |  | |  |  | | --- | --- | | ****Name:**** | **Macor** | | ****Model type:**** | **Linear Elastic Isotropic** | | ****Default failure criterion:**** | **Unknown** | | ****Yield strength:**** | **3.3e+07 N/m^2** | | ****Tensile strength:**** | **3.3e+07 N/m^2** | | ****Compressive strength:**** | **3.45e+08 N/m^2** | | ****Elastic modulus:**** | **6.69e+10 N/m^2** | | ****Poisson's ratio:**** | **0.29** | | ****Mass density:**** | **2,520 kg/m^3** | | ****Shear modulus:**** | **2.55e+10 N/m^2** | | ****Thermal expansion coefficient:**** | **8e-06 /Kelvin** | | **SolidBody 1(CirPattern2)(bplate\_simplified\_compression\_borderless-1)** | | **Curve Data:N/A** | | | |  | |  |  | | --- | --- | | ****Name:**** | **Kapton HN** | | ****Model type:**** | **Linear Elastic Isotropic** | | ****Default failure criterion:**** | **Unknown** | | ****Yield strength:**** | **6.9e+07 N/m^2** | | ****Tensile strength:**** | **2.31e+08 N/m^2** | | ****Compressive strength:**** | **2.31e+08 N/m^2** | | ****Elastic modulus:**** | **2.76e+09 N/m^2** | | ****Poisson's ratio:**** | **0.34** | | ****Mass density:**** | **1,420 kg/m^3** | | ****Thermal expansion coefficient:**** | **20 /Kelvin** | | **SolidBody 1(Boss-Extrude1)(pcb\_simplified\_nofillet-1),**  **SolidBody 1(Fillet1)(separation\_layer\_simplified-1)** | | **Curve Data:N/A** | | | |  | |  |  | | --- | --- | | ****Name:**** | **FR4** | | ****Model type:**** | **Linear Elastic Isotropic** | | ****Default failure criterion:**** | **Unknown** | | ****Yield strength:**** | **3.45e+08 N/m^2** | | ****Tensile strength:**** | **3.45e+08 N/m^2** | | ****Compressive strength:**** | **3.5e+08 N/m^2** | | ****Elastic modulus:**** | **2.156e+10 N/m^2** | | ****Poisson's ratio:**** | **0.136** | | ****Mass density:**** | **2,000 kg/m^3** | | **SolidBody 1(Fillet1)(power\_supply\_pcb\_mockup\_v4.2-1)** | | **Curve Data:N/A** | | | |  | |  |  | | --- | --- | | ****Name:**** | **Alumina** | | ****Model type:**** | **Linear Elastic Isotropic** | | ****Default failure criterion:**** | **Unknown** | | ****Tensile strength:**** | **3e+08 N/m^2** | | ****Compressive strength:**** | **3e+09 N/m^2** | | ****Elastic modulus:**** | **3.7e+11 N/m^2** | | ****Poisson's ratio:**** | **0.22** | | ****Mass density:**** | **3,960 kg/m^3** | | ****Shear modulus:**** | **1.5e+11 N/m^2** | | ****Thermal expansion coefficient:**** | **7e-06 /Kelvin** | | **SolidBody 1(Split Line1)(tplate\_simplified-1)** | | **Curve Data:N/A** | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Loads and Fixtures**  | ****Fixture name**** | ****Fixture Image**** | ****Fixture Details**** | | --- | --- | --- | | **Fixed-1** |  | |  |  | | --- | --- | | Entities: | **1 face(s)** | | Type: | **Fixed Geometry** | | | ****Resultant Forces****   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Components** | **X** | **Y** | **Z** | **Resultant** | | **Reaction force(N)** | **-4.36265e-05** | **486** | **-3.31608e-05** | **486** | | **Reaction Moment(N.m)** | **0** | **0** | **0** | **0** | | | |  | ****Load name**** | ****Load Image**** | ****Load Details**** | | --- | --- | --- | | **Force-1** |  | |  |  | | --- | --- | | Entities: | **1 face(s)** | | Type: | **Apply normal force** | | Value: | **486 N** | | |

|  |
| --- |
| Connector Definitions No Data |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Contact Information  | Contact | Contact Image | Contact Properties | | --- | --- | --- | | Contact Set-1 |  | |  |  | | --- | --- | | Type: | **Bonded contact pair** | | Entities: | **2 face(s)** | | | ****Contact/Friction force****   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Components** | **X** | **Y** | **Z** | **Resultant** | | **Contact Force(N)** | **0** | **12.474** | **0** | **12.474** | | | | | Contact Set-2 |  | |  |  | | --- | --- | | Type: | **Bonded contact pair** | | Entities: | **2 face(s)** | | | ****Contact/Friction force****   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Components** | **X** | **Y** | **Z** | **Resultant** | | **Contact Force(N)** | **0** | **62.21** | **0** | **62.21** | | | | | Contact Set-3 |  | |  |  | | --- | --- | | Type: | **Bonded contact pair** | | Entities: | **2 face(s)** | | | ****Contact/Friction force****   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Components** | **X** | **Y** | **Z** | **Resultant** | | **Contact Force(N)** | **-1.8691E-16** | **-14.81** | **-4.5073E-07** | **14.81** | | | | | Contact Set-4 |  | |  |  | | --- | --- | | Type: | **Bonded contact pair** | | Entities: | **10 face(s)** | | | ****Contact/Friction force****   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Components** | **X** | **Y** | **Z** | **Resultant** | | **Contact Force(N)** | **-1.5094** | **52.284** | **-2.2859** | **52.356** | | | | | Component Contact-1 |  | |  |  | | --- | --- | | Type: | **No penetration (Surface to surface)** | | Components: | **7 component(s)** | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Mesh information  |  |  | | --- | --- | | Mesh type | Solid Mesh | | Mesher Used: | Standard mesh | | Automatic Transition: | Off | | Include Mesh Auto Loops: | Off | | Jacobian points | 4 Points | | Element Size | 0.2 in | | Tolerance | 0.01 in | | Mesh Quality Plot | High | | Remesh failed parts with incompatible mesh | Off |  Mesh information - Details  |  |  | | --- | --- | | Total Nodes | 85690 | | Total Elements | 46949 | | Maximum Aspect Ratio | 182.12 | | % of elements with Aspect Ratio < 3 | 31.3 | | % of elements with Aspect Ratio > 10 | 49.6 | | % of distorted elements(Jacobian) | 0 | | Time to complete mesh(hh;mm;ss): | 00:00:13 | | Computer name: | THICCO | |  | |  Mesh Control Information:  | **Mesh Control Name** | **Mesh Control Image** | **Mesh Control Details** | | --- | --- | --- | | **Control-1** |  | |  |  | | --- | --- | | Entities: | **2 Solid Body (s)** | | Units: | **in** | | Size: | **0.195** | | Ratio: | **0.195** | | |

|  |
| --- |
| Sensor Details No Data |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Resultant ForcesReaction forces  | Selection set | Units | Sum X | Sum Y | Sum Z | Resultant | | --- | --- | --- | --- | --- | --- | | Entire Model | N | -4.36265e-05 | 486 | -3.31608e-05 | 486 |  Reaction Moments  | Selection set | Units | Sum X | Sum Y | Sum Z | Resultant | | --- | --- | --- | --- | --- | --- | | Entire Model | N.m | 0 | 0 | 0 | 0 | |
|  |

|  |
| --- |
| Beams No Data |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Study Results  | Name | Type | Min | Max | | --- | --- | --- | --- | | Stress1 | VON: von Mises Stress | 1.029e-01 N/m^2  Node: 46449 | 1.071e+08 N/m^2  Node: 73126 | | **borderless\_simplified\_panel\_compression-compression-Stress-Stress1** | | | |  | Name | Type | Min | Max | | --- | --- | --- | --- | | Displacement1 | URES: Resultant Displacement | 0.000e+00 mm  Node: 28218 | 2.715e-01 mm  Node: 862 | | **borderless\_simplified\_panel\_compression-compression-Displacement-Displacement1** | | | |  | Name | Type | Min | Max | | --- | --- | --- | --- | | Strain1 | ESTRN: Equivalent Strain | 1.830e-12  Element: 25084 | 1.445e-03  Element: 37703 | | **borderless\_simplified\_panel\_compression-compression-Strain-Strain1** | | | |  | Name | Type | Min | Max | | --- | --- | --- | --- | | Factor of Safety1 | Mohr-Coulomb Stress | 2.975e+00  Node: 78228 | 3.000e+00  Node: 1 | | **borderless\_simplified\_panel\_compression-compression-Factor of Safety-Factor of Safety1** | | | | |

|  |
| --- |
| Conclusion |